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Description automatically generated with low confidence]X Adventure Forces 
Blak/Black/Black (L45482300)

The X Adventure Forces is a product from the Salomon Forces line. This model is NOT  ISO 20347 : 2022 certified. This document serves to simplify the understanding of how the product is constructed. 

  	Product Reference:			X ADVENTURE FORCES
  	Article Code:				L45482300
	Color: 					Blak/Black/Black
	Construction & Material of Outsole:	Cemented EVA Midsole / Rubber Outsole
		






                     		
	Manufacturer:				Salomon SA
						ZA des Croiselets
						14 Chemin des Croiselets
						74370 Epagny, Metz Tessy
						France

		

Product Description: 
The X ADVENTURE FORCES is a modern and lightweight shoe.
The upper material needs to be robust and very flexible. To meet these requirements, a non-reflective material mix of coated synthetic and knitwear stretch has been selected. The toe cap protects the foot from shocks and ensures high comfort. The Quicklace™ is a fast-lacing system to provide a secure, precise and almost customized fit. 
The performance and stability of the sole construction play a crucial role. In combination, the Contagrip® MA outsole, Advanced Chassis™ and EnergyCell damping meet all performance requirements. An OrthoLite® inlay sole ensures a comfortable fit and additional damping in the boot.
The X ADENTURE FORCES is a perfect choice for anyone looking for a comfortable low-cut shoe.

Size Range: 
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Product Technology Highlights: 
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	Technologies / Material
	Description

	Coated Synthetic Leather
	Coated Synthetic Leather of 1.3mm thickness
A coated synthetic non woven backer that protects it and makes it stronger to last longer.

	Non-reflective materials
	Built to be discrete and non-reflective for Tactical use.

	Lace Pocket
	Tuck the excess lace and the buckle up inside the pocket on the tongue of the shoe.

	QuicklaceTM Laces
	Minimalistic and strong lace for one-pull tightening. Easy-on, easy-off.

	Protective Toecap
	3D Toecap construction

	Advanced Chassis™
	Advanced Chassis™ is a molded insert embedded in the outsole. Providing strong lateral support and reassuring protection, it also delivers optimal mobility and flexibility.

	EnergyCell
	A high-rebound midsole compound that provides exceptional energy return along with substantial cushioning and durability. 

	OrthoLite® 
Insole
	Ortholite® insoles provide step-in comfort and enhanced durability, breathability, moisture and odor control using a combination of special PU and rubber

	Contagrip® 
Outsole
	Developed using All Terrain Contagrip, for adhesion and confidence on the widest variety of surfaces. 
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Sockliner Dimensions: 
Ortholite – Molded single piece
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*Made without intentionally added per- & polyFlucrinated substances: may contain unintended trace amounts.
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Reference Material Thickness (mm) Weight (g/m²) Color

HMD 3706 SL 0.6MM (toebox) Needle Punch With Hot Melt 0.6 Black

S7500T 1.3MM (toecap)

Coated Synthetic Non Woven 

Backer

1.3 Black

S7500T 1.3MM 

Coated Synthetic Non Woven 

Backer

1.3 Black

ET W5281 (pocket) Sandwich Mesh Black

S7500T 1.3MM 

Coated Synthetic Non Woven 

Backer

1.3 Black

Eyelet JS 7050-CB-CU-7X4X5MM Metal Black

Lining ET L5236 Knitwear Stretch Type 1 Way Black

Insole DOUBLE TEX 25 0.8MM RE 100% Stitch Bonded Black

Midsole 024 52C IM EVA  Black

Chassis

SLMFT139 – CHASSIS – COVESTRO - 

UTECHLLAN TPU – 95A

INJECTED PIECE Plastic soft 

(Shore A)

Black

Outsole 60A 80HT EVOLUTION Rubber Black

Upper

Tongue
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